(kicad_pcb (version 4) (host pcbnew 0.201507310902+6023~28~ubuntu14.04.1-product)
  (general
    (links 356)
    (no_connects 0)
    (area 74.944999 81.849999 199.045001 119.950001)
    (thickness 1.6)
    (drawings 59)
    (tracks 1792)
    (zones 0)
    (modules 144)
    (nets 103)
  )
  (page A4)
  (layers
    (0 F.Cu-L1 signal)
    (1 L2-GND signal)
    (2 L3-PWR signal)
    (31 B.Cu-L4 signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.3048)
    (user_trace_width 0.254)
    (user_trace_width 0.4064)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (user_trace_width 1.016)
    (user_trace_width 1.27)
    (trace_clearance 0.2286)
    (zone_clearance 0.5)
    (zone_45_only no)
    (trace_min 0.2032)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.9144)
    (via_drill 0.4064)
    (via_min_size 0.4572)
    (via_min_drill 0.3048)
    (user_via 0.762 0.4572)
    (user_via 1.1176 0.6096)
    (user_via 1.2192 0.7112)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.1)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 2)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 74.995 119.9)
    (grid_origin 74.995 119.9)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000007)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerber/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 Vdd)
  (net 4 "Net-(C14-Pad1)")
  (net 5 AVdd)
  (net 6 "Net-(C16-Pad2)")
  (net 7 V+)
  (net 8 V-)
  (net 9 SCK)
  (net 10 SCL)
  (net 11 SDA)
  (net 12 SDO)
  (net 13 "Net-(R28-Pad2)")
  (net 14 "Net-(C11-Pad1)")
  (net 15 "Net-(C14-Pad2)")
  (net 16 "Net-(C15-Pad1)")
  (net 17 "Net-(C16-Pad1)")
  (net 18 "Net-(C18-Pad2)")
  (net 19 VR-)
  (net 20 "Net-(C23-Pad1)")
  (net 21 "Net-(C23-Pad2)")
  (net 22 VR+)
  (net 23 "Net-(C29-Pad1)")
  (net 24 "Net-(C29-Pad2)")
  (net 25 "Net-(R16-Pad1)")
  (net 26 CH1out)
  (net 27 CH2out)
  (net 28 CH3out)
  (net 29 "Net-(R46-Pad1)")
  (net 30 MIC)
  (net 31 MICout)
  (net 32 "Net-(C6-Pad2)")
  (net 33 "Net-(C30-Pad2)")
  (net 34 SQ4)
  (net 35 CH1)
  (net 36 CH2)
  (net 37 CH3)
  (net 38 "Net-(R22-Pad1)")
  (net 39 "Net-(R33-Pad2)")
  (net 40 "Net-(U11-Pad3)")
  (net 41 CS.CH2)
  (net 42 CS.CH1)
  (net 43 "Net-(R14-Pad2)")
  (net 44 "Net-(U10-Pad6)")
  (net 45 "Net-(D3-Pad2)")
  (net 46 WG1)
  (net 47 SQR1)
  (net 48 SEN)
  (net 49 CAP)
  (net 50 Rg)
  (net 51 /D-)
  (net 52 /D+)
  (net 53 "Net-(C5-Pad1)")
  (net 54 /SQ2)
  (net 55 "Net-(D1-Pad2)")
  (net 56 "Net-(D2-Pad1)")
  (net 57 "Net-(C25-Pad1)")
  (net 58 12MHz)
  (net 59 PV1)
  (net 60 PV2)
  (net 61 ID1)
  (net 62 "Net-(R37-Pad2)")
  (net 63 /SQ1)
  (net 64 "Net-(C3-Pad1)")
  (net 65 "Net-(C24-Pad1)")
  (net 66 "Net-(C33-Pad1)")
  (net 67 "Net-(C36-Pad1)")
  (net 68 WG2)
  (net 69 "Net-(R19-Pad2)")
  (net 70 "Net-(R21-Pad2)")
  (net 71 "Net-(C40-Pad2)")
  (net 72 PDC2)
  (net 73 "Net-(Q1-Pad1)")
  (net 74 "Net-(Q1-Pad2)")
  (net 75 CCS)
  (net 76 "Net-(R27-Pad2)")
  (net 77 "Net-(C41-Pad1)")
  (net 78 "Net-(C42-Pad1)")
  (net 79 /SQ3)
  (net 80 RB14)
  (net 81 "Net-(R7-Pad2)")
  (net 82 "Net-(R15-Pad2)")
  (net 83 /OD1)
  (net 84 BOD1)
  (net 85 "Net-(C45-Pad1)")
  (net 86 "Net-(R52-Pad1)")
  (net 87 /PGC2)
  (net 88 "Net-(R51-Pad1)")
  (net 89 "Net-(C3-Pad2)")
  (net 90 SQR2)
  (net 91 "Net-(D4-Pad2)")
  (net 92 SQ4B)
  (net 93 SQ4A)
  (net 94 RB15)
  (net 95 AN8)
  (net 96 VUSB)
  (net 97 "Net-(R55-Pad1)")
  (net 98 RXD)
  (net 99 TXD)
  (net 100 MCLR)
  (net 101 "Net-(C7-Pad1)")
  (net 102 /PGD2)
  (net_class Default "This is the default net class."
    (clearance 0.2286)
    (trace_width 0.3048)
    (via_dia 0.9144)
    (via_drill 0.4064)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +5V)
    (add_net /D+)
    (add_net /D-)
    (add_net /OD1)
    (add_net /PGC2)
    (add_net /PGD2)
    (add_net /SQ1)
    (add_net /SQ2)
    (add_net /SQ3)
    (add_net 12MHz)
    (add_net AN8)
    (add_net AVdd)
    (add_net BOD1)
    (add_net CAP)
    (add_net CCS)
    (add_net CH1)
    (add_net CH1out)
    (add_net CH2)
    (add_net CH2out)
    (add_net CH3)
    (add_net CH3out)
    (add_net CS.CH1)
    (add_net CS.CH2)
    (add_net GND)
    (add_net ID1)
    (add_net MCLR)
    (add_net MIC)
    (add_net MICout)
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C14-Pad2)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C16-Pad2)")
    (add_net "Net-(C18-Pad2)")
    (add_net "Net-(C23-Pad1)")
    (add_net "Net-(C23-Pad2)")
    (add_net "Net-(C24-Pad1)")
    (add_net "Net-(C25-Pad1)")
    (add_net "Net-(C29-Pad1)")
    (add_net "Net-(C29-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C30-Pad2)")
    (add_net "Net-(C33-Pad1)")
    (add_net "Net-(C36-Pad1)")
    (add_net "Net-(C40-Pad2)")
    (add_net "Net-(C41-Pad1)")
    (add_net "Net-(C42-Pad1)")
    (add_net "Net-(C45-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(R14-Pad2)")
    (add_net "Net-(R15-Pad2)")
    (add_net "Net-(R16-Pad1)")
    (add_net "Net-(R19-Pad2)")
    (add_net "Net-(R21-Pad2)")
    (add_net "Net-(R22-Pad1)")
    (add_net "Net-(R27-Pad2)")
    (add_net "Net-(R28-Pad2)")
    (add_net "Net-(R33-Pad2)")
    (add_net "Net-(R37-Pad2)")
    (add_net "Net-(R46-Pad1)")
    (add_net "Net-(R51-Pad1)")
    (add_net "Net-(R52-Pad1)")
    (add_net "Net-(R55-Pad1)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(U10-Pad6)")
    (add_net "Net-(U11-Pad3)")
    (add_net PDC2)
    (add_net PV1)
    (add_net PV2)
    (add_net RB14)
    (add_net RB15)
    (add_net RXD)
    (add_net Rg)
    (add_net SCK)
    (add_net SCL)
    (add_net SDA)
    (add_net SDO)
    (add_net SEN)
    (add_net SQ4)
    (add_net SQ4A)
    (add_net SQ4B)
    (add_net SQR1)
    (add_net SQR2)
    (add_net TXD)
    (add_net V+)
    (add_net V-)
    (add_net VR+)
    (add_net VR-)
    (add_net VUSB)
    (add_net Vdd)
    (add_net WG1)
    (add_net WG2)
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 58438025)
    (at 118.745 98.5 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0.05 -1.45 90) (layer F.SilkS))
    (fp_text value 0.1u (at -0.05 0.05 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 3 Vdd))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 57DD1611)
    (at 111 115 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at -2.4 0.125 90) (layer F.SilkS))
    (fp_text value 0.1u (at 2.455 0.535 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 64 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 89 "Net-(C3-Pad2)"))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 5843BA73)
    (at 150.695 97.275)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at -0.025 1.6 180) (layer F.SilkS))
    (fp_text value 0.1u (at -0.05 0.05) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 0) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 3 Vdd))
    (pad 2 smd rect (at 1 0) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 58522452)
    (at 193.095 114.78 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at -2.455 -0.025 450) (layer F.SilkS))
    (fp_text value 1u (at -0.05 0.05 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 53 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 30 MIC))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 58510904)
    (at 135.245 114.95 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at -2.5 0.575 90) (layer F.SilkS))
    (fp_text value 10nF (at -3 -0.475 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 101 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 5821AB80)
    (at 104.895 90.4 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 2.15 0 360) (layer F.SilkS))
    (fp_text value 0.1u (at -0.05 0.05 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 2 +5V))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 582158FA)
    (at 99.795 115.05 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 2.8 -0.05 450) (layer F.SilkS))
    (fp_text value 0.1u (at -3.1 0.475 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 8 V-))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:TantalC_SizeC_EIA-6032_Reflow (layer F.Cu-L1) (tedit 5821509C)
    (at 88.645 101.3 180)
    (descr "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (tags "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (attr smd)
    (fp_text reference C11 (at 4.8 0.2 450) (layer F.SilkS))
    (fp_text value 100u (at 0.48 -0.05 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 2.52476 0 180) (size 2.55016 2.49936) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.52476 0 180) (size 2.55016 2.49936) (layers F.Cu-L1 F.Paste F.Mask)
      (net 14 "Net-(C11-Pad1)"))
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 584A3877)
    (at 139.245 85.95 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C13 (at 0.025 -1.525 270) (layer F.SilkS))
    (fp_text value 0.1u (at -0.05 0.05 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 3 Vdd))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:TantalC_SizeC_EIA-6032_Reflow (layer F.Cu-L1) (tedit 5821509E)
    (at 88.67 96.8 180)
    (descr "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (tags "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (attr smd)
    (fp_text reference C14 (at 4.8 0 270) (layer F.SilkS))
    (fp_text value 100u (at 0.48 -0.05 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 2.52476 0 180) (size 2.55016 2.49936) (layers F.Cu-L1 F.Paste F.Mask)
      (net 15 "Net-(C14-Pad2)"))
    (pad 1 smd rect (at -2.52476 0 180) (size 2.55016 2.49936) (layers F.Cu-L1 F.Paste F.Mask)
      (net 4 "Net-(C14-Pad1)"))
  )
  (module MyLib:TantalC_SizeC_EIA-6032_Reflow (layer F.Cu-L1) (tedit 58512DF8)
    (at 80.42 113.15 180)
    (descr "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (tags "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (attr smd)
    (fp_text reference C16 (at 4.825 -0.025 450) (layer F.SilkS))
    (fp_text value 100u (at 0.48 -0.05 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 2.52476 0 180) (size 2.55016 2.49936) (layers F.Cu-L1 F.Paste F.Mask)
      (net 6 "Net-(C16-Pad2)"))
    (pad 1 smd rect (at -2.52476 0 180) (size 2.55016 2.49936) (layers F.Cu-L1 F.Paste F.Mask)
      (net 17 "Net-(C16-Pad1)"))
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 58438308)
    (at 140.145 107.85 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C17 (at -2.8 -0.2 90) (layer F.SilkS))
    (fp_text value 0.1u (at -0.05 0.05 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 5 AVdd))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:TantalC_SizeC_EIA-6032_Reflow (layer F.Cu-L1) (tedit 58512DFE)
    (at 80.445 116.825 180)
    (descr "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (tags "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (attr smd)
    (fp_text reference C18 (at 4.8 0 450) (layer F.SilkS))
    (fp_text value 100u (at 0.48 -0.05 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 2.52476 0 180) (size 2.55016 2.49936) (layers F.Cu-L1 F.Paste F.Mask)
      (net 18 "Net-(C18-Pad2)"))
    (pad 1 smd rect (at -2.52476 0 180) (size 2.55016 2.49936) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 58441B12)
    (at 171.02 88.25 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C20 (at 2.95 0.525 90) (layer F.SilkS))
    (fp_text value 1u (at 2.4 -0.475 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 2 +5V))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 582A90D3)
    (at 179.395 115 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C22 (at -2.77 0.32 270) (layer F.SilkS))
    (fp_text value 0.1u (at -0.05 0.05 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 19 VR-))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 582A931F)
    (at 156.395 115 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C23 (at 2.81 0.5 270) (layer F.SilkS))
    (fp_text value 3p3 (at 2.74 -0.56 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 20 "Net-(C23-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 21 "Net-(C23-Pad2)"))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 582AF78C)
    (at 118.045 115 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C24 (at 2.75 0.4 450) (layer F.SilkS))
    (fp_text value 0.1u (at -0.05 0.05 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 65 "Net-(C24-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 58512B0D)
    (at 168.52 116.3)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C25 (at 0 1.625 180) (layer F.SilkS))
    (fp_text value 0.1u (at -0.05 0.05) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 0) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 57 "Net-(C25-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 35 CH1))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 57FB2655)
    (at 155.945 107.3 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C26 (at -2.875 0.15 270) (layer F.SilkS))
    (fp_text value 0.1u (at -0.05 0.05 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 22 VR+))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 5821A593)
    (at 108.545 106.2 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C27 (at 2.75 0.05 90) (layer F.SilkS))
    (fp_text value 0.1u (at -2.975 0.625 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 7 V+))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 5833AD5B)
    (at 189.245 115.05 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C28 (at -2.75 -0.25 90) (layer F.SilkS))
    (fp_text value 0.1u (at -0.05 0.05 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 19 VR-))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 58018081)
    (at 172.47 115 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C29 (at 2.65 0.6 270) (layer F.SilkS))
    (fp_text value 3p3 (at 2.625 -0.375 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 23 "Net-(C29-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 24 "Net-(C29-Pad2)"))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 57FB601B)
    (at 172.685 108.22 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C31 (at -2.75 0.075 90) (layer F.SilkS))
    (fp_text value 0.1u (at -0.05 0.05 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 22 VR+))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 57D650F0)
    (at 172.545 96.3 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C32 (at 2.85 -0.05 90) (layer F.SilkS))
    (fp_text value 0.1u (at -0.05 0.05 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 5 AVdd))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 57D64632)
    (at 163.595 114.95 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C34 (at -2.9 0 270) (layer F.SilkS))
    (fp_text value 0.1u (at -0.05 0.05 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 19 VR-))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 5843803E)
    (at 122.645 105.7 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C35 (at -2.85 -0.05 450) (layer F.SilkS))
    (fp_text value 0.1u (at 0.1 -0.05 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 7 V+))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:MountingHole-clear (layer F.Cu-L1) (tedit 559D0EEF)
    (at 78.995 100.9)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference MH1 (at 0.1 -3.3) (layer F.SilkS) hide)
    (fp_text value M (at 0 -0.32) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.5) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
  )
  (module MyLib:MountingHole-clear locked (layer F.Cu-L1) (tedit 559D0EEF)
    (at 191.045 100.925)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference MH2 (at 0.1 -3.3) (layer F.SilkS) hide)
    (fp_text value M (at 0 -0.32) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.5) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 584A3887)
    (at 156.395 86.15 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -0.225 -2.7 270) (layer F.SilkS))
    (fp_text value 10K (at -0.075 -1.625 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 3 Vdd))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 100 MCLR))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 584388A6)
    (at 194.995 94.975 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 2.35 0.55 90) (layer F.SilkS))
    (fp_text value 10K (at 2.8 -0.5 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 10 SCL))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 3 Vdd))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 58443601)
    (at 192.245 94.95 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 3.175 -0.5 90) (layer F.SilkS))
    (fp_text value 10K (at 2.85 0.5 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 11 SDA))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 3 Vdd))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 584383C2)
    (at 143.245 107.85 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 2.35 -0.55 450) (layer F.SilkS))
    (fp_text value 1K (at 2.45 0.45 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 7 V+))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 55 "Net-(D1-Pad2)"))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 57DCA3DC)
    (at 115.745 115 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 2.5 0.5 270) (layer F.SilkS))
    (fp_text value 10K (at 2.75 -0.55 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 65 "Net-(C24-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 64 "Net-(C3-Pad1)"))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 5812B380)
    (at 113.3 115 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at -2.375 -0.525 90) (layer F.SilkS))
    (fp_text value 10K (at -2.725 0.425 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 64 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 81 "Net-(R7-Pad2)"))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 584A3866)
    (at 123.775 99.54 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at -2.39 0.53 270) (layer F.SilkS))
    (fp_text value 5K1 (at -2.79 -0.52 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 45 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 95 AN8))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 585129BA)
    (at 142.37 114.925 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 2.8 -0.7 270) (layer F.SilkS))
    (fp_text value 10K (at 2.8 0.475 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 94 RB15))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 49 CAP))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 58438418)
    (at 144.92 114.925 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 2.7 -0.55 450) (layer F.SilkS))
    (fp_text value 1K (at 2.55 0.45 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 8 V-))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 56 "Net-(D2-Pad1)"))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 57D65266)
    (at 153.725 100.52 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at -2.75 -0.45 270) (layer F.SilkS))
    (fp_text value 5K1 (at -2.8 0.6 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 5 AVdd))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 48 SEN))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 57D650BF)
    (at 167.895 96.3 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R16 (at 2.8 0.5 90) (layer F.SilkS))
    (fp_text value 10K (at 2.8 -0.6 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 25 "Net-(R16-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 5 AVdd))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 5833AC2F)
    (at 167.895 100.87 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R17 (at -0.17 2.55 270) (layer F.SilkS))
    (fp_text value 10K (at -0.02 1.5 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 25 "Net-(R16-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 5821A3B7)
    (at 120.295 109.95 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R18 (at 2.75 -0.55 270) (layer F.SilkS))
    (fp_text value 10K (at 2.75 0.5 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 67 "Net-(C36-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 66 "Net-(C33-Pad1)"))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 58215E15)
    (at 106.145 106.25 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R19 (at -2.85 -0.55 270) (layer F.SilkS))
    (fp_text value 10K (at -2.95 0.5 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 5 AVdd))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 69 "Net-(R19-Pad2)"))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 57D63520)
    (at 158.545 115 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R20 (at 2.75 -0.65 270) (layer F.SilkS))
    (fp_text value 200K (at 3.1 0.4 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 20 "Net-(C23-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 21 "Net-(C23-Pad2)"))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 57FB2681)
    (at 165.595 96.3 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R22 (at 2.775 0.475 90) (layer F.SilkS))
    (fp_text value 10K (at 2.775 -0.55 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 38 "Net-(R22-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 5 AVdd))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 57FB2687)
    (at 155.945 100.5 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R23 (at -2.75 -0.55 270) (layer F.SilkS))
    (fp_text value 10K (at -2.775 0.475 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 38 "Net-(R22-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 20 "Net-(C23-Pad1)"))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 57DBE1D7)
    (at 161.345 114.95 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R24 (at 2.75 -0.55 270) (layer F.SilkS))
    (fp_text value 1M (at 2.425 0.425 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 57 "Net-(C25-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 21 "Net-(C23-Pad2)"))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 58215903)
    (at 97.395 115.1 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R25 (at -2.8 0.9 90) (layer F.SilkS))
    (fp_text value 10K (at -3.4 -0.1 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 77 "Net-(C41-Pad1)"))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 582158C8)
    (at 94.845 115.1 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R26 (at -2.7 0.55 90) (layer F.SilkS))
    (fp_text value 5K1 (at -2.7 -0.65 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 77 "Net-(C41-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 59 PV1))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 585109D4)
    (at 121.47 115.675 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R27 (at -2.725 0.475 90) (layer F.SilkS))
    (fp_text value 10K (at -2.75 -0.575 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 46 WG1))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 76 "Net-(R27-Pad2)"))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 5821EE1B)
    (at 172.425 100.9 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R28 (at -2.87 0.605 90) (layer F.SilkS))
    (fp_text value 10K (at -2.96 -0.47 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 23 "Net-(C29-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 13 "Net-(R28-Pad2)"))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 57D650C5)
    (at 170.295 96.3 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R29 (at -2.8 -0.6 270) (layer F.SilkS))
    (fp_text value 10K (at -2.7 0.45 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 5 AVdd))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 13 "Net-(R28-Pad2)"))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 58521935)
    (at 174.695 115 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R30 (at 2.725 -0.425 270) (layer F.SilkS))
    (fp_text value 200K (at 3.075 0.55 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 23 "Net-(C29-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 24 "Net-(C29-Pad2)"))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 582BE1E6)
    (at 183.27 93.675 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R31 (at 2.925 -0.425 90) (layer F.SilkS))
    (fp_text value 10K (at 2.8 0.55 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 31 MICout))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 5 AVdd))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 57959D6A)
    (at 181.095 93.675 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R32 (at 2.85 -0.71 90) (layer F.SilkS))
    (fp_text value 10K (at 2.825 0.315 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 28 CH3out))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 5 AVdd))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 582A8D71)
    (at 181.695 115.05 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R33 (at 2.78 0.48 270) (layer F.SilkS))
    (fp_text value 10K (at 2.73 -0.52 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 28 CH3out))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 39 "Net-(R33-Pad2)"))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 58521940)
    (at 176.995 115 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R34 (at -2.9 0.625 90) (layer F.SilkS))
    (fp_text value 1M (at -3.25 -0.425 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 36 CH2))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 24 "Net-(C29-Pad2)"))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 5843803A)
    (at 122.645 109.9 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R35 (at -2.8 0.4 90) (layer F.SilkS))
    (fp_text value 10K (at -2.8 -0.6 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 76 "Net-(R27-Pad2)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 68 WG2))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 5833AD31)
    (at 153.945 115.025 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R37 (at 0.1 2.63 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.61 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 61 ID1))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 62 "Net-(R37-Pad2)"))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 582C2EFE)
    (at 183.995 115.05 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R38 (at 2.85 0.45 270) (layer F.SilkS))
    (fp_text value 10K (at 2.85 -0.65 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 50 Rg))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 39 "Net-(R33-Pad2)"))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 57DB9152)
    (at 185.52 93.7 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R39 (at 2.95 0.575 90) (layer F.SilkS))
    (fp_text value 10K (at 2.95 -0.475 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 30 MIC))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 5 AVdd))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 585109E3)
    (at 127.395 114.925 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R41 (at 2.8 0.475 270) (layer F.SilkS))
    (fp_text value 5K1 (at 2.75 -0.575 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 33 "Net-(C30-Pad2)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 101 "Net-(C7-Pad1)"))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 585106EA)
    (at 129.645 114.95 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R42 (at 2.775 -0.65 270) (layer F.SilkS))
    (fp_text value 10K (at 2.8 0.375 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 101 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 46 WG1))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 5842A062)
    (at 140.145 114.95 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R43 (at 2.8 -0.6 270) (layer F.SilkS))
    (fp_text value 5K1 (at 2.75 0.45 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 92 SQ4B))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 582D3099)
    (at 186.895 115.05 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R45 (at -2.8 0.5 90) (layer F.SilkS))
    (fp_text value 10M (at -2.8 -0.55 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 37 CH3))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 582C3073)
    (at 188.745 107.425 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R46 (at -2.875 -0.5 90) (layer F.SilkS))
    (fp_text value 200K (at -3.175 0.55 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 29 "Net-(R46-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 43 "Net-(R14-Pad2)"))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 57DB90CA)
    (at 191.37 107.45 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R47 (at 2.75 -0.6 270) (layer F.SilkS))
    (fp_text value 1K (at 2.4 0.45 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 29 "Net-(R46-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 53 "Net-(C5-Pad1)"))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:myTestPoint (layer F.Cu-L1) (tedit 5784421D)
    (at 163.92 95.5)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference TP1 (at 1.275 1.125) (layer F.SilkS) hide)
    (fp_text value AVdd (at 0.225 1.885) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 5 AVdd))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:myTestPoint (layer F.Cu-L1) (tedit 578489B3)
    (at 97.815 86.72)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference TP2 (at 2.05 -0.1) (layer F.SilkS) hide)
    (fp_text value Vdd (at 0.03 -1.54) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.6096) (layers *.Cu *.Mask F.SilkS)
      (net 3 Vdd))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:TQFP-44 (layer F.Cu-L1) (tedit 585218EA)
    (at 140.595 96)
    (attr smd)
    (fp_text reference U3 (at -8.2 -5.2) (layer F.SilkS))
    (fp_text value PIC24EP64GP204 (at -0.2 1.85 180) (layer F.SilkS))
    (pad 39 smd rect (at 0 -5.715) (size 0.4064 1.524) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 40 smd rect (at -0.8001 -5.715) (size 0.4064 1.524) (layers F.Cu-L1 F.Paste F.Mask)
      (net 3 Vdd))
    (pad 41 smd rect (at -1.6002 -5.715) (size 0.4064 1.524) (layers F.Cu-L1 F.Paste F.Mask)
      (net 102 /PGD2))
    (pad 42 smd rect (at -2.4003 -5.715) (size 0.4064 1.524) (layers F.Cu-L1 F.Paste F.Mask)
      (net 87 /PGC2))
    (pad 43 smd rect (at -3.2004 -5.715) (size 0.4064 1.524) (layers F.Cu-L1 F.Paste F.Mask)
      (net 98 RXD))
    (pad 44 smd rect (at -4.0005 -5.715) (size 0.4064 1.524) (layers F.Cu-L1 F.Paste F.Mask)
      (net 99 TXD))
    (pad 38 smd rect (at 0.8001 -5.715) (size 0.4064 1.524) (layers F.Cu-L1 F.Paste F.Mask))
    (pad 37 smd rect (at 1.6002 -5.715) (size 0.4064 1.524) (layers F.Cu-L1 F.Paste F.Mask))
    (pad 36 smd rect (at 2.4003 -5.715) (size 0.4064 1.524) (layers F.Cu-L1 F.Paste F.Mask)
      (net 9 SCK))
    (pad 35 smd rect (at 3.2004 -5.715) (size 0.4064 1.524) (layers F.Cu-L1 F.Paste F.Mask))
    (pad 34 smd rect (at 4.0005 -5.715) (size 0.4064 1.524) (layers F.Cu-L1 F.Paste F.Mask)
      (net 12 SDO))
    (pad 17 smd rect (at 0 5.715) (size 0.4064 1.524) (layers F.Cu-L1 F.Paste F.Mask)
      (net 5 AVdd))
    (pad 16 smd rect (at -0.8001 5.715) (size 0.4064 1.524) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 15 smd rect (at -1.6002 5.715) (size 0.4064 1.524) (layers F.Cu-L1 F.Paste F.Mask)
      (net 94 RB15))
    (pad 14 smd rect (at -2.4003 5.715) (size 0.4064 1.524) (layers F.Cu-L1 F.Paste F.Mask)
      (net 80 RB14))
    (pad 13 smd rect (at -3.2004 5.715) (size 0.4064 1.524) (layers F.Cu-L1 F.Paste F.Mask)
      (net 41 CS.CH2))
    (pad 12 smd rect (at -4.0005 5.715) (size 0.4064 1.524) (layers F.Cu-L1 F.Paste F.Mask)
      (net 42 CS.CH1))
    (pad 18 smd rect (at 0.8001 5.715) (size 0.4064 1.524) (layers F.Cu-L1 F.Paste F.Mask)
      (net 100 MCLR))
    (pad 19 smd rect (at 1.6002 5.715) (size 0.4064 1.524) (layers F.Cu-L1 F.Paste F.Mask)
      (net 27 CH2out))
    (pad 20 smd rect (at 2.4003 5.715) (size 0.4064 1.524) (layers F.Cu-L1 F.Paste F.Mask)
      (net 28 CH3out))
    (pad 21 smd rect (at 3.2004 5.715) (size 0.4064 1.524) (layers F.Cu-L1 F.Paste F.Mask)
      (net 31 MICout))
    (pad 22 smd rect (at 4.0005 5.715) (size 0.4064 1.524) (layers F.Cu-L1 F.Paste F.Mask)
      (net 26 CH1out))
    (pad 6 smd rect (at -5.715 0) (size 1.524 0.4064) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 28 smd rect (at 5.715 0) (size 1.524 0.4064) (layers F.Cu-L1 F.Paste F.Mask)
      (net 3 Vdd))
    (pad 7 smd rect (at -5.715 0.8001) (size 1.524 0.4064) (layers F.Cu-L1 F.Paste F.Mask)
      (net 16 "Net-(C15-Pad1)"))
    (pad 27 smd rect (at 5.715 0.8001) (size 1.524 0.4064) (layers F.Cu-L1 F.Paste F.Mask)
      (net 95 AN8))
    (pad 26 smd rect (at 5.715 1.6002) (size 1.524 0.4064) (layers F.Cu-L1 F.Paste F.Mask)
      (net 48 SEN))
    (pad 8 smd rect (at -5.715 1.6002) (size 1.524 0.4064) (layers F.Cu-L1 F.Paste F.Mask)
      (net 93 SQ4A))
    (pad 9 smd rect (at -5.715 2.4003) (size 1.524 0.4064) (layers F.Cu-L1 F.Paste F.Mask)
      (net 92 SQ4B))
    (pad 25 smd rect (at 5.715 2.4003) (size 1.524 0.4064) (layers F.Cu-L1 F.Paste F.Mask)
      (net 75 CCS))
    (pad 24 smd rect (at 5.715 3.2004) (size 1.524 0.4064) (layers F.Cu-L1 F.Paste F.Mask)
      (net 49 CAP))
    (pad 10 smd rect (at -5.715 3.2004) (size 1.524 0.4064) (layers F.Cu-L1 F.Paste F.Mask)
      (net 83 /OD1))
    (pad 11 smd rect (at -5.715 4.0005) (size 1.524 0.4064) (layers F.Cu-L1 F.Paste F.Mask)
      (net 63 /SQ1))
    (pad 23 smd rect (at 5.715 4.0005) (size 1.524 0.4064) (layers F.Cu-L1 F.Paste F.Mask)
      (net 62 "Net-(R37-Pad2)"))
    (pad 29 smd rect (at 5.715 -0.8001) (size 1.524 0.4064) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -5.715 -0.8001) (size 1.524 0.4064) (layers F.Cu-L1 F.Paste F.Mask)
      (net 34 SQ4))
    (pad 4 smd rect (at -5.715 -1.6002) (size 1.524 0.4064) (layers F.Cu-L1 F.Paste F.Mask)
      (net 79 /SQ3))
    (pad 30 smd rect (at 5.715 -1.6002) (size 1.524 0.4064) (layers F.Cu-L1 F.Paste F.Mask)
      (net 85 "Net-(C45-Pad1)"))
    (pad 31 smd rect (at 5.715 -2.4003) (size 1.524 0.4064) (layers F.Cu-L1 F.Paste F.Mask)
      (net 58 12MHz))
    (pad 3 smd rect (at -5.715 -2.4003) (size 1.524 0.4064) (layers F.Cu-L1 F.Paste F.Mask)
      (net 54 /SQ2))
    (pad 2 smd rect (at -5.715 -3.2004) (size 1.524 0.4064) (layers F.Cu-L1 F.Paste F.Mask)
      (net 83 /OD1))
    (pad 32 smd rect (at 5.715 -3.2004) (size 1.524 0.4064) (layers F.Cu-L1 F.Paste F.Mask)
      (net 11 SDA))
    (pad 33 smd rect (at 5.715 -4.0005) (size 1.524 0.4064) (layers F.Cu-L1 F.Paste F.Mask)
      (net 10 SCL))
    (pad 1 smd rect (at -5.715 -4.0005) (size 1.524 0.4064) (layers F.Cu-L1 F.Paste F.Mask)
      (net 63 /SQ1))
    (model smd/tqfp44.wrl
      (at (xyz 0 0 0))
      (scale (xyz 4 4 4))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:SOT-23-6 (layer F.Cu-L1) (tedit 5821576B)
    (at 90.245 90.65 270)
    (fp_text reference U4 (at -2.2 0 540) (layer F.SilkS))
    (fp_text value TC1240A (at 2.21 0.01 360) (layer F.SilkS) hide)
    (pad 6 smd rect (at -0.9525 -1.27 270) (size 0.70104 1.00076) (layers F.Cu-L1 F.Paste F.Mask)
      (net 4 "Net-(C14-Pad1)"))
    (pad 5 smd rect (at 0 -1.27 270) (size 0.70104 1.00076) (layers F.Cu-L1 F.Paste F.Mask)
      (net 14 "Net-(C11-Pad1)"))
    (pad 4 smd rect (at 0.9525 -1.27 270) (size 0.70104 1.00076) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.9525 1.27 270) (size 0.70104 1.00076) (layers F.Cu-L1 F.Paste F.Mask)
      (net 15 "Net-(C14-Pad2)"))
    (pad 2 smd rect (at 0 1.27 270) (size 0.70104 1.00076) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 1.27 270) (size 0.70104 1.00076) (layers F.Cu-L1 F.Paste F.Mask)
      (net 2 +5V))
    (model smd/SOT23_6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.11 0.11 0.11))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 584430E0)
    (at 182.095 101 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C37 (at -2.75 0.225 270) (layer F.SilkS))
    (fp_text value 0.1u (at -0.05 0.05 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 22 VR+))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 58437EF6)
    (at 131.87 114.95 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C38 (at -2.75 0.175 270) (layer F.SilkS))
    (fp_text value 0.1u (at -0.05 0.05 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 8 V-))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 57D648C2)
    (at 184.495 101 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at -2.75 0.4 270) (layer F.SilkS))
    (fp_text value 10K (at -2.75 -0.55 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 31 MICout))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 43 "Net-(R14-Pad2)"))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 5842792E)
    (at 124.02 115.65 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C30 (at -2.8 0.545 90) (layer F.SilkS))
    (fp_text value 1nF (at -2.85 -0.505 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 46 WG1))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 33 "Net-(C30-Pad2)"))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 584A3871)
    (at 135.345 85.95 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at -2.425 -0.6 270) (layer F.SilkS))
    (fp_text value 5K1 (at -2.825 0.425 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 91 "Net-(D4-Pad2)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 3 Vdd))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 5843C8C4)
    (at 156.57 94.05 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C39 (at 0.75 -1.45 270) (layer F.SilkS))
    (fp_text value 0.1u (at -0.05 0.05 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 5 AVdd))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 5844150E)
    (at 132.995 85.95 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference D4 (at 0.85 1.6 90) (layer F.SilkS) hide)
    (fp_text value LED (at 2.6 0.05 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 91 "Net-(D4-Pad2)"))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:myTestPoint (layer F.Cu-L1) (tedit 57DD19F8)
    (at 85.615 83.65)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference TP4 (at -1.82 0.88) (layer F.SilkS) hide)
    (fp_text value Vusb (at 1.8 0.1) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.778 1.778) (drill 0.7112) (layers *.Cu *.Mask F.SilkS)
      (net 96 VUSB))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:SOT-223 (layer F.Cu-L1) (tedit 582151FA)
    (at 98.545 87.85 90)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U6 (at -3.15 -4.825 180) (layer F.SilkS))
    (fp_text value LM1117-3.3 (at -0.0738 0.3697 90) (layer F.SilkS) hide)
    (pad 4 smd rect (at 0 -3.302 90) (size 3.6576 2.032) (layers F.Cu-L1 F.Paste F.Mask)
      (net 3 Vdd))
    (pad 2 smd rect (at 0 3.302 90) (size 1.016 2.032) (layers F.Cu-L1 F.Paste F.Mask)
      (net 3 Vdd))
    (pad 3 smd rect (at 2.286 3.302 90) (size 1.016 2.032) (layers F.Cu-L1 F.Paste F.Mask)
      (net 2 +5V))
    (pad 1 smd rect (at -2.286 3.302 90) (size 1.016 2.032) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (model smd/SOT223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module TRAN:sot23 (layer F.Cu-L1) (tedit 58441B33)
    (at 167.495 88.2 180)
    (descr SOT23)
    (attr smd)
    (fp_text reference U15 (at -0.625 3.15 270) (layer F.SilkS))
    (fp_text value 3033 (at 0.425 3.525 450) (layer F.SilkS))
    (pad 1 smd rect (at -0.9525 1.05664 180) (size 0.59944 1.00076) (layers F.Cu-L1 F.Paste F.Mask)
      (net 2 +5V))
    (pad 3 smd rect (at 0 -1.05664 180) (size 0.59944 1.00076) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.9525 1.05664 180) (size 0.59944 1.00076) (layers F.Cu-L1 F.Paste F.Mask)
      (net 5 AVdd))
    (model smd/smd_transistors/sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer F.Cu-L1) (tedit 584908BC)
    (at 111.245 87.7 90)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at -4.4 -3.82 360) (layer F.SilkS))
    (fp_text value 74HC126 (at -0.45 0.85 180) (layer F.SilkS))
    (pad 1 smd rect (at -2.7 -3.81 90) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at -2.7 -2.54 90) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 63 /SQ1))
    (pad 3 smd rect (at -2.7 -1.27 90) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 88 "Net-(R51-Pad1)"))
    (pad 4 smd rect (at -2.7 0 90) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 2 +5V))
    (pad 5 smd rect (at -2.7 1.27 90) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 83 /OD1))
    (pad 6 smd rect (at -2.7 2.54 90) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 84 BOD1))
    (pad 7 smd rect (at -2.7 3.81 90) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 2.7 3.81 90) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 84 BOD1))
    (pad 9 smd rect (at 2.7 2.54 90) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 83 /OD1))
    (pad 10 smd rect (at 2.7 1.27 90) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 2 +5V))
    (pad 11 smd rect (at 2.7 0 90) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 90 SQR2))
    (pad 12 smd rect (at 2.7 -1.27 90) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 87 /PGC2))
    (pad 13 smd rect (at 2.7 -2.54 90) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 2 +5V))
    (pad 14 smd rect (at 2.7 -3.81 90) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 2 +5V))
    (model Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu-L1) (tedit 58512EAF)
    (at 80.42 107.775)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U5 (at -4.275 -1.875 270) (layer F.SilkS))
    (fp_text value 7660 (at 5.01 -0.65 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 17 "Net-(C16-Pad1)"))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 6 "Net-(C16-Pad2)"))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 18 "Net-(C18-Pad2)"))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 14 "Net-(C11-Pad1)"))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu-L1) (tedit 57DD1685)
    (at 160.5 108 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U8 (at -4.475 -1.955 360) (layer F.SilkS))
    (fp_text value TL082 (at 1.025 0.445 180) (layer F.SilkS))
    (pad 1 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 20 "Net-(C23-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 21 "Net-(C23-Pad2)"))
    (pad 3 smd rect (at -2.7 0.635 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -2.7 1.905 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 19 VR-))
    (pad 5 smd rect (at 2.7 1.905 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 25 "Net-(R16-Pad1)"))
    (pad 6 smd rect (at 2.7 0.635 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 40 "Net-(U11-Pad3)"))
    (pad 7 smd rect (at 2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 40 "Net-(U11-Pad3)"))
    (pad 8 smd rect (at 2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 22 VR+))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:SOIC-8_3.9x4.9mm_Pitch1.27mm locked (layer F.Cu-L1) (tedit 57DD168A)
    (at 177 108 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U10 (at -4.5 -1.63 180) (layer F.SilkS))
    (fp_text value TL082 (at 0 0.095 180) (layer F.SilkS))
    (pad 1 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 23 "Net-(C29-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 24 "Net-(C29-Pad2)"))
    (pad 3 smd rect (at -2.7 0.635 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -2.7 1.905 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 19 VR-))
    (pad 5 smd rect (at 2.7 1.905 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 25 "Net-(R16-Pad1)"))
    (pad 6 smd rect (at 2.7 0.635 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 44 "Net-(U10-Pad6)"))
    (pad 7 smd rect (at 2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 44 "Net-(U10-Pad6)"))
    (pad 8 smd rect (at 2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 22 VR+))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu-L1) (tedit 585218E4)
    (at 160.5 98 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U11 (at -4.525 0.02 360) (layer F.SilkS))
    (fp_text value 6S21 (at -0.325 0.17 180) (layer F.SilkS))
    (pad 1 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 26 CH1out))
    (pad 2 smd rect (at -2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 38 "Net-(R22-Pad1)"))
    (pad 3 smd rect (at -2.7 0.635 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 40 "Net-(U11-Pad3)"))
    (pad 4 smd rect (at -2.7 1.905 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 2.7 1.905 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 42 CS.CH1))
    (pad 6 smd rect (at 2.7 0.635 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 12 SDO))
    (pad 7 smd rect (at 2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 9 SCK))
    (pad 8 smd rect (at 2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 5 AVdd))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu-L1) (tedit 585218DC)
    (at 177 98 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U12 (at -4.45 -1.605 360) (layer F.SilkS))
    (fp_text value 6S21 (at 0.075 0.095 180) (layer F.SilkS))
    (pad 1 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 27 CH2out))
    (pad 2 smd rect (at -2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 13 "Net-(R28-Pad2)"))
    (pad 3 smd rect (at -2.7 0.635 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 44 "Net-(U10-Pad6)"))
    (pad 4 smd rect (at -2.7 1.905 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 2.7 1.905 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 41 CS.CH2))
    (pad 6 smd rect (at 2.7 0.635 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 12 SDO))
    (pad 7 smd rect (at 2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 9 SCK))
    (pad 8 smd rect (at 2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 5 AVdd))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu-L1) (tedit 5800589A)
    (at 127.5 108 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U13 (at -4.45 -1.63 180) (layer F.SilkS))
    (fp_text value TL082 (at 0.425 0.22 180) (layer F.SilkS))
    (pad 1 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 46 WG1))
    (pad 2 smd rect (at -2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 33 "Net-(C30-Pad2)"))
    (pad 3 smd rect (at -2.7 0.635 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -2.7 1.905 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 8 V-))
    (pad 5 smd rect (at 2.7 1.905 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.7 0.635 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 76 "Net-(R27-Pad2)"))
    (pad 7 smd rect (at 2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 68 WG2))
    (pad 8 smd rect (at 2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 7 V+))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:PICKIT-PROG (layer F.Cu-L1) (tedit 57859DFD)
    (at 148.745 86.25 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 7.175 0.215 180) (layer F.SilkS) hide)
    (fp_text value prog (at 0.3 1.8 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -5.08 0 180) (size 1.27 1.27) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 100 MCLR))
    (pad 2 thru_hole circle (at -2.54 0 180) (size 1.27 1.27) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 3 Vdd))
    (pad 3 thru_hole circle (at 0 0 180) (size 1.27 1.27) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 4 thru_hole circle (at 2.54 0 180) (size 1.27 1.27) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 102 /PGD2))
    (pad 5 thru_hole circle (at 5.08 0 180) (size 1.27 1.27) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 87 /PGC2))
    (model Pin_Headers/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 5821AAE8)
    (at 104.895 86 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 2.6 0.55 90) (layer F.SilkS))
    (fp_text value 1u (at 2.5 -0.6 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 2 +5V))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:Fuse-1206-1812 (layer F.Cu-L1) (tedit 582A8AE1)
    (at 89.795 84.4)
    (descr "Capacitor SMD 1812, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1812")
    (attr smd)
    (fp_text reference F1 (at 0.17 2.49) (layer F.SilkS))
    (fp_text value 0.5A (at -0.025 -0.075 270) (layer F.SilkS))
    (pad 1 smd rect (at -2.3 0) (size 1 3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 96 VUSB))
    (pad 2 smd rect (at 2.3 0) (size 1 3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 2 +5V))
    (pad 1 smd rect (at -1.5 0) (size 0.6 2) (layers F.Cu-L1 F.Paste F.Mask)
      (net 96 VUSB))
    (pad 2 smd rect (at 1.5 0) (size 0.6 2) (layers F.Cu-L1 F.Paste F.Mask)
      (net 2 +5V))
    (model Capacitors_SMD/C_1812P.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:xtl-3225 (layer F.Cu-L1) (tedit 584F7F49)
    (at 152.02 93.975)
    (descr "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (tags "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (attr smd)
    (fp_text reference U14 (at -2.825 -0.7 90) (layer F.SilkS))
    (fp_text value XTL-4pin (at 0.3 2.9 180) (layer F.SilkS) hide)
    (pad 4 smd rect (at -1.1 -0.85) (size 1.4 1.2) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 0.85) (size 1.4 1.2) (layers F.Cu-L1 F.Paste F.Mask)
      (net 85 "Net-(C45-Pad1)"))
    (pad 2 smd rect (at 1.1 0.85) (size 1.4 1.2) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.1 -0.85) (size 1.4 1.2) (layers F.Cu-L1 F.Paste F.Mask)
      (net 58 12MHz))
  )
  (module MyLib:SOT-23-EBC (layer F.Cu-L1) (tedit 58512896)
    (at 151.82 106.25 270)
    (descr "Module CMS SOT23 Transistore EBC")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference Q3 (at -3.35 -0.175 360) (layer F.SilkS))
    (fp_text value 3904 (at -2.25 -0.575 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.889 -1.016 270) (size 0.9144 0.9144) (layers F.Cu-L1 F.Paste F.Mask)
      (net 22 VR+))
    (pad 2 smd rect (at 0.889 -1.016 270) (size 0.9144 0.9144) (layers F.Cu-L1 F.Paste F.Mask)
      (net 55 "Net-(D1-Pad2)"))
    (pad 3 smd rect (at 0 1.016 270) (size 0.9144 0.9144) (layers F.Cu-L1 F.Paste F.Mask)
      (net 7 V+))
    (model smd/cms_sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.15 0.15))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:mySwitch-3way (layer F.Cu-L1) (tedit 58510E1F)
    (at 168 109 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference SW1 (at 0 -2.286 270) (layer F.SilkS) hide)
    (fp_text value sw (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -3 0 270) (size 2.2 1.7) (drill oval 1.8 1) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at 0 0 270) (size 2.2 1.7) (drill oval 1.7 1) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(C25-Pad1)"))
    (pad 3 thru_hole oval (at 3 0 270) (size 2.2 1.7) (drill oval 1.8 1) (layers *.Cu *.Mask F.SilkS)
      (net 35 CH1))
    (model Pin_Headers/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:SOT-23-zener (layer F.Cu-L1) (tedit 5843868E)
    (at 147.52 106.175 270)
    (descr "Module CMS SOT23 Transistore EBC")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference D1 (at -1.5 1.255 360) (layer F.SilkS))
    (fp_text value 6v8 (at -2.55 -0.075 360) (layer F.SilkS))
    (pad 3 smd rect (at -0.889 -1.016 270) (size 0.9144 0.9144) (layers F.Cu-L1 F.Paste F.Mask))
    (pad 1 smd rect (at 0.889 -1.016 270) (size 0.9144 0.9144) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 1.016 270) (size 0.9144 0.9144) (layers F.Cu-L1 F.Paste F.Mask)
      (net 55 "Net-(D1-Pad2)"))
    (model smd/cms_sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.15 0.15))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:SOT-23-zener (layer F.Cu-L1) (tedit 58512AB8)
    (at 147.52 111.225 270)
    (descr "Module CMS SOT23 Transistore EBC")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference D2 (at 3.375 -0.025 540) (layer F.SilkS))
    (fp_text value 6v8 (at 2.275 -0.05 540) (layer F.SilkS))
    (pad 3 smd rect (at -0.889 -1.016 270) (size 0.9144 0.9144) (layers F.Cu-L1 F.Paste F.Mask))
    (pad 1 smd rect (at 0.889 -1.016 270) (size 0.9144 0.9144) (layers F.Cu-L1 F.Paste F.Mask)
      (net 56 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0 1.016 270) (size 0.9144 0.9144) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (model smd/cms_sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.15 0.15))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu-L1) (tedit 582BE021)
    (at 184 108 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U9 (at -2.9 -3.255 90) (layer F.SilkS))
    (fp_text value TL082 (at -0.55 0.545 180) (layer F.SilkS))
    (pad 1 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 39 "Net-(R33-Pad2)"))
    (pad 2 smd rect (at -2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 50 Rg))
    (pad 3 smd rect (at -2.7 0.635 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 37 CH3))
    (pad 4 smd rect (at -2.7 1.905 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 19 VR-))
    (pad 5 smd rect (at 2.7 1.905 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.7 0.635 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 29 "Net-(R46-Pad1)"))
    (pad 7 smd rect (at 2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 43 "Net-(R14-Pad2)"))
    (pad 8 smd rect (at 2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 22 VR+))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:speaker-header-14-small locked (layer B.Cu-L4) (tedit 58006B59)
    (at 108 117 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -21.32 -0.9 270) (layer B.SilkS))
    (fp_text value outputs (at 2 3 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at 19.25 0) (size 1.5 3) (layers B.Cu-L4 B.Paste B.Mask)
      (net 75 CCS))
    (pad 12 smd rect (at -19.25 0) (size 1.5 3) (layers B.Cu-L4 B.Paste B.Mask)
      (net 46 WG1))
    (pad 2 smd rect (at 15.75 0) (size 1.5 3) (layers B.Cu-L4 B.Paste B.Mask)
      (net 59 PV1))
    (pad 3 smd rect (at 12.25 0) (size 1.5 3) (layers B.Cu-L4 B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 8.75 0) (size 1.5 3) (layers B.Cu-L4 B.Paste B.Mask)
      (net 60 PV2))
    (pad 5 smd rect (at 5.25 0) (size 1.5 3) (layers B.Cu-L4 B.Paste B.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 1.75 0) (size 1.5 3) (layers B.Cu-L4 B.Paste B.Mask)
      (net 47 SQR1))
    (pad 7 smd rect (at -1.75 0) (size 1.5 3) (layers B.Cu-L4 B.Paste B.Mask)
      (net 1 GND))
    (pad 8 smd rect (at -5.25 0) (size 1.5 3) (layers B.Cu-L4 B.Paste B.Mask)
      (net 90 SQR2))
    (pad 9 smd rect (at -8.75 0) (size 1.5 3) (layers B.Cu-L4 B.Paste B.Mask)
      (net 1 GND))
    (pad 10 smd rect (at -12.25 0) (size 1.5 3) (layers B.Cu-L4 B.Paste B.Mask)
      (net 84 BOD1))
    (pad 11 smd rect (at -15.75 0) (size 1.5 3) (layers B.Cu-L4 B.Paste B.Mask)
      (net 68 WG2))
    (model Pin_Headers/Pin_Header_Straight_1x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:speaker-header-14-small locked (layer B.Cu-L4) (tedit 582A90DD)
    (at 172 117)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at 21.255 1.28) (layer B.SilkS))
    (fp_text value Inputs (at 2 3) (layer B.SilkS) hide)
    (pad 1 smd rect (at 19.25 0 180) (size 1.5 3) (layers B.Cu-L4 B.Paste B.Mask)
      (net 30 MIC))
    (pad 12 smd rect (at -19.25 0 180) (size 1.5 3) (layers B.Cu-L4 B.Paste B.Mask)
      (net 49 CAP))
    (pad 2 smd rect (at 15.75 0 180) (size 1.5 3) (layers B.Cu-L4 B.Paste B.Mask)
      (net 50 Rg))
    (pad 3 smd rect (at 12.25 0 180) (size 1.5 3) (layers B.Cu-L4 B.Paste B.Mask)
      (net 37 CH3))
    (pad 4 smd rect (at 8.75 0 180) (size 1.5 3) (layers B.Cu-L4 B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 5.25 0 180) (size 1.5 3) (layers B.Cu-L4 B.Paste B.Mask)
      (net 36 CH2))
    (pad 6 smd rect (at 1.75 0 180) (size 1.5 3) (layers B.Cu-L4 B.Paste B.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -1.75 0 180) (size 1.5 3) (layers B.Cu-L4 B.Paste B.Mask)
      (net 35 CH1))
    (pad 8 smd rect (at -5.25 0 180) (size 1.5 3) (layers B.Cu-L4 B.Paste B.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -8.75 0 180) (size 1.5 3) (layers B.Cu-L4 B.Paste B.Mask)
      (net 48 SEN))
    (pad 10 smd rect (at -12.25 0 180) (size 1.5 3) (layers B.Cu-L4 B.Paste B.Mask)
      (net 1 GND))
    (pad 11 smd rect (at -15.75 0 180) (size 1.5 3) (layers B.Cu-L4 B.Paste B.Mask)
      (net 61 ID1))
    (model Pin_Headers/Pin_Header_Straight_1x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 5821A382)
    (at 118.045 110 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C33 (at -0.05 -1.4 90) (layer F.SilkS))
    (fp_text value 0.1u (at 0.5 1.5 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 66 "Net-(C33-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 72 PDC2))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 58438028)
    (at 118.045 105.7 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C36 (at 2.8 -0.1 90) (layer F.SilkS))
    (fp_text value 0.1u (at 0.3 -0.05 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 67 "Net-(C36-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 58438053)
    (at 120.295 105.75 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R15 (at 2.75 -0.5 90) (layer F.SilkS))
    (fp_text value 10K (at 2.8 0.5 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 66 "Net-(C33-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 82 "Net-(R15-Pad2)"))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 5829B2FC)
    (at 106.145 110.55 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R21 (at -2.56 0.63 90) (layer F.SilkS))
    (fp_text value 10K (at -2.7 -0.35 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 69 "Net-(R19-Pad2)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 70 "Net-(R21-Pad2)"))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu-L1) (tedit 58512CE0)
    (at 113 108 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U7 (at -4.375 -1.955 180) (layer F.SilkS))
    (fp_text value TL082 (at 0.53 0.425 180) (layer F.SilkS))
    (pad 1 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 89 "Net-(C3-Pad2)"))
    (pad 2 smd rect (at -2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 89 "Net-(C3-Pad2)"))
    (pad 3 smd rect (at -2.7 0.635 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 65 "Net-(C24-Pad1)"))
    (pad 4 smd rect (at -2.7 1.905 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 8 V-))
    (pad 5 smd rect (at 2.7 1.905 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 67 "Net-(C36-Pad1)"))
    (pad 6 smd rect (at 2.7 0.635 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 72 PDC2))
    (pad 7 smd rect (at 2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 72 PDC2))
    (pad 8 smd rect (at 2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 7 V+))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:SOIC-16_3.9x9.9mm_Pitch1.27mm (layer B.Cu-L4) (tedit 57DD1669)
    (at 124.395 93.3 270)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 4.5 -4.525 540) (layer B.SilkS))
    (fp_text value CH340G (at -0.075 0.175 540) (layer B.SilkS) hide)
    (pad 1 smd rect (at -2.7 4.445 270) (size 1.5 0.6) (layers B.Cu-L4 B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.7 3.175 270) (size 1.5 0.6) (layers B.Cu-L4 B.Paste B.Mask)
      (net 99 TXD))
    (pad 3 smd rect (at -2.7 1.905 270) (size 1.5 0.6) (layers B.Cu-L4 B.Paste B.Mask)
      (net 98 RXD))
    (pad 4 smd rect (at -2.7 0.635 270) (size 1.5 0.6) (layers B.Cu-L4 B.Paste B.Mask)
      (net 3 Vdd))
    (pad 5 smd rect (at -2.7 -0.635 270) (size 1.5 0.6) (layers B.Cu-L4 B.Paste B.Mask)
      (net 52 /D+))
    (pad 6 smd rect (at -2.7 -1.905 270) (size 1.5 0.6) (layers B.Cu-L4 B.Paste B.Mask)
      (net 51 /D-))
    (pad 7 smd rect (at -2.7 -3.175 270) (size 1.5 0.6) (layers B.Cu-L4 B.Paste B.Mask)
      (net 58 12MHz))
    (pad 8 smd rect (at -2.7 -4.445 270) (size 1.5 0.6) (layers B.Cu-L4 B.Paste B.Mask))
    (pad 9 smd rect (at 2.7 -4.445 270) (size 1.5 0.6) (layers B.Cu-L4 B.Paste B.Mask))
    (pad 10 smd rect (at 2.7 -3.175 270) (size 1.5 0.6) (layers B.Cu-L4 B.Paste B.Mask))
    (pad 11 smd rect (at 2.7 -1.905 270) (size 1.5 0.6) (layers B.Cu-L4 B.Paste B.Mask))
    (pad 12 smd rect (at 2.7 -0.635 270) (size 1.5 0.6) (layers B.Cu-L4 B.Paste B.Mask))
    (pad 13 smd rect (at 2.7 0.635 270) (size 1.5 0.6) (layers B.Cu-L4 B.Paste B.Mask))
    (pad 14 smd rect (at 2.7 1.905 270) (size 1.5 0.6) (layers B.Cu-L4 B.Paste B.Mask))
    (pad 15 smd rect (at 2.7 3.175 270) (size 1.5 0.6) (layers B.Cu-L4 B.Paste B.Mask))
    (pad 16 smd rect (at 2.7 4.445 270) (size 1.5 0.6) (layers B.Cu-L4 B.Paste B.Mask)
      (net 3 Vdd))
    (model Housings_SOIC.3dshapes/SOIC-16_3.9x9.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:myPin_Header_Straight_1x02 (layer F.Cu-L1) (tedit 57DBB7CF)
    (at 80 95.075)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference D3 (at -3.775 -0.2 90) (layer F.SilkS))
    (fp_text value LED (at 0.3 1.8) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -1.27 0) (size 1.7272 1.7272) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.7272 1.7272) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(D3-Pad2)"))
    (model Pin_Headers/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer F.Cu-L1) (tedit 57FF7EDE)
    (at 99.6 108 270)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U16 (at 4.475 3.4 360) (layer F.SilkS))
    (fp_text value LM324 (at -0.175 0.22 360) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.7 -3.81 270) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 60 PV2))
    (pad 2 smd rect (at -2.7 -2.54 270) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 71 "Net-(C40-Pad2)"))
    (pad 3 smd rect (at -2.7 -1.27 270) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 72 PDC2))
    (pad 4 smd rect (at -2.7 0 270) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 7 V+))
    (pad 5 smd rect (at -2.7 1.27 270) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 80 RB14))
    (pad 6 smd rect (at -2.7 2.54 270) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 73 "Net-(Q1-Pad1)"))
    (pad 7 smd rect (at -2.7 3.81 270) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 74 "Net-(Q1-Pad2)"))
    (pad 8 smd rect (at 2.7 3.81 270) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 59 PV1))
    (pad 9 smd rect (at 2.7 2.54 270) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 77 "Net-(C41-Pad1)"))
    (pad 10 smd rect (at 2.7 1.27 270) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 70 "Net-(R21-Pad2)"))
    (pad 11 smd rect (at 2.7 0 270) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 8 V-))
    (pad 12 smd rect (at 2.7 -1.27 270) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 78 "Net-(C42-Pad1)"))
    (pad 13 smd rect (at 2.7 -2.54 270) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 69 "Net-(R19-Pad2)"))
    (pad 14 smd rect (at 2.7 -3.81 270) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 70 "Net-(R21-Pad2)"))
    (model Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 582155EC)
    (at 103.145 99.15)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R36 (at -2.75 -0.4) (layer F.SilkS))
    (fp_text value 10K (at -2.8 0.55) (layer F.SilkS))
    (pad 1 smd rect (at -1 0) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 71 "Net-(C40-Pad2)"))
    (pad 2 smd rect (at 1 0) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 60 PV2))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:SOT-23-EBC (layer F.Cu-L1) (tedit 58512D7F)
    (at 87.945 116.5)
    (descr "Module CMS SOT23 Transistore EBC")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference Q1 (at -1.85 1.025) (layer F.SilkS))
    (fp_text value 3906 (at 0.175 2.15) (layer F.SilkS))
    (pad 1 smd rect (at -0.889 -1.016) (size 0.9144 0.9144) (layers F.Cu-L1 F.Paste F.Mask)
      (net 73 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.889 -1.016) (size 0.9144 0.9144) (layers F.Cu-L1 F.Paste F.Mask)
      (net 74 "Net-(Q1-Pad2)"))
    (pad 3 smd rect (at 0 1.016) (size 0.9144 0.9144) (layers F.Cu-L1 F.Paste F.Mask)
      (net 75 CCS))
    (model smd/cms_sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.15 0.15))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 57DCEA2D)
    (at 97.195 96.8)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R48 (at -2.725 0.55) (layer F.SilkS))
    (fp_text value 1K (at -2.75 -0.475) (layer F.SilkS))
    (pad 1 smd rect (at -1 0) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 73 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 5 AVdd))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 5833AD80)
    (at 103.145 101.5 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C40 (at 2.7 -0.15 180) (layer F.SilkS))
    (fp_text value 0.1u (at 0.5 1.5 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 0 180) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 60 PV2))
    (pad 2 smd rect (at 1 0 180) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 71 "Net-(C40-Pad2)"))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 57DCEA20)
    (at 97.195 99.15 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R40 (at 2.75 -0.575 180) (layer F.SilkS))
    (fp_text value 5K1 (at 2.725 0.475 180) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 180) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 5 AVdd))
    (pad 2 smd rect (at 1 0 180) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 80 RB14))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 5848E04F)
    (at 97.195 101.55)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R44 (at -2.82 0.34) (layer F.SilkS))
    (fp_text value 10K (at -2.84 -0.62) (layer F.SilkS))
    (pad 1 smd rect (at -1 0) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 80 RB14))
    (pad 2 smd rect (at 1 0) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 5821584C)
    (at 92.495 115.1 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C41 (at -2.9 0 90) (layer F.SilkS))
    (fp_text value 0.1u (at 0.5 1.5 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 77 "Net-(C41-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 59 PV1))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 57DD2264)
    (at 102.135 115.08 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C42 (at 2.775 0.05 270) (layer F.SilkS))
    (fp_text value 0.1u (at 0.5 1.5 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 78 "Net-(C42-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 58215D54)
    (at 104.415 115.07 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R49 (at -2.75 -0.5 90) (layer F.SilkS))
    (fp_text value 10K (at -2.75 0.45 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 89 "Net-(C3-Pad2)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 78 "Net-(C42-Pad1)"))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 58215325)
    (at 103.145 96.8 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R50 (at 2.75 0.6 180) (layer F.SilkS))
    (fp_text value 10K (at 2.8 -0.5 180) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 180) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 5 AVdd))
    (pad 2 smd rect (at 1 0 180) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 71 "Net-(C40-Pad2)"))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:myPin_Header_Straight_1x08-oval (layer F.Cu-L1) (tedit 580078C2)
    (at 196 108 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P6 (at 11.325 -0.025 360) (layer F.SilkS))
    (fp_text value exp (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -8.89 0 270) (size 1.7272 1.7272) (drill 0.9144) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 2 thru_hole oval (at -6.35 0 270) (size 1.7272 1.9304) (drill 0.9144) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at -3.81 0 270) (size 1.7272 1.9304) (drill 0.9144) (layers *.Cu *.Mask F.SilkS)
      (net 10 SCL))
    (pad 4 thru_hole oval (at -1.27 0 270) (size 1.7272 1.9304) (drill 0.9144) (layers *.Cu *.Mask F.SilkS)
      (net 11 SDA))
    (pad 5 thru_hole oval (at 1.27 0 270) (size 1.7272 1.9304) (drill 0.9144) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 thru_hole oval (at 3.81 0 270) (size 1.7272 1.9304) (drill 0.9144) (layers *.Cu *.Mask F.SilkS)
      (net 22 VR+))
    (pad 7 thru_hole oval (at 6.35 0 270) (size 1.7272 1.9304) (drill 0.9144) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 8 thru_hole oval (at 8.89 0 270) (size 1.7272 1.9304) (drill 0.9144) (layers *.Cu *.Mask F.SilkS)
      (net 19 VR-))
    (model Pin_Headers/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer F.Cu-L1) (tedit 5849083E)
    (at 111.145 97.7 90)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U17 (at -2.67 -5.2 90) (layer F.SilkS))
    (fp_text value 74HC126 (at 0.08 1.21 180) (layer F.SilkS))
    (pad 1 smd rect (at -2.7 -3.81 90) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 5 AVdd))
    (pad 2 smd rect (at -2.7 -2.54 90) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 54 /SQ2))
    (pad 3 smd rect (at -2.7 -1.27 90) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 81 "Net-(R7-Pad2)"))
    (pad 4 smd rect (at -2.7 0 90) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 5 AVdd))
    (pad 5 smd rect (at -2.7 1.27 90) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 79 /SQ3))
    (pad 6 smd rect (at -2.7 2.54 90) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 82 "Net-(R15-Pad2)"))
    (pad 7 smd rect (at -2.7 3.81 90) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 2.7 3.81 90) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask))
    (pad 9 smd rect (at 2.7 2.54 90) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 2.7 1.27 90) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 2.7 0 90) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask))
    (pad 12 smd rect (at 2.7 -1.27 90) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 13 smd rect (at 2.7 -2.54 90) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 14 smd rect (at 2.7 -3.81 90) (size 1.5 0.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 5 AVdd))
    (model Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:SOT-23-EBC (layer F.Cu-L1) (tedit 58512A62)
    (at 151.77 111.2 270)
    (descr "Module CMS SOT23 Transistore EBC")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference Q2 (at -1.5 1.45 360) (layer F.SilkS))
    (fp_text value 3906 (at -2.4 -1 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.889 -1.016 270) (size 0.9144 0.9144) (layers F.Cu-L1 F.Paste F.Mask)
      (net 19 VR-))
    (pad 2 smd rect (at 0.889 -1.016 270) (size 0.9144 0.9144) (layers F.Cu-L1 F.Paste F.Mask)
      (net 56 "Net-(D2-Pad1)"))
    (pad 3 smd rect (at 0 1.016 270) (size 0.9144 0.9144) (layers F.Cu-L1 F.Paste F.Mask)
      (net 8 V-))
    (model smd/cms_sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.15 0.15))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 5848F36E)
    (at 103.145 93.85 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C43 (at 2.66 0.49 180) (layer F.SilkS))
    (fp_text value 0.1u (at 0.5 1.5 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 0 180) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 5 AVdd))
    (pad 2 smd rect (at 1 0 180) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:my-4pin-smd (layer F.Cu-L1) (tedit 584A38DC)
    (at 194.345 84.075)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at -5.4 1.225 180) (layer F.SilkS))
    (fp_text value USB2 (at 5.5 0 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at -1 0) (size 1.2 3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 51 /D-))
    (pad 3 smd rect (at 1 0) (size 1.2 3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 52 /D+))
    (pad 4 smd rect (at 3 0) (size 1.5 3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -3 0) (size 1.5 3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 96 VUSB))
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 5829B450)
    (at 108.525 110.56 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R51 (at 2.73 -0.77 270) (layer F.SilkS))
    (fp_text value 100 (at 3.18 0.16 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 88 "Net-(R51-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 47 SQR1))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:SOIC-20-W (layer F.Cu-L1) (tedit 5848F28F)
    (at 124.445 89.65)
    (attr smd)
    (fp_text reference U18 (at -7.475 4.475 90) (layer F.SilkS))
    (fp_text value MCP2200 (at -0.05 -2.11) (layer F.SilkS))
    (pad 1 smd rect (at -5.715 5) (size 0.762 1.27) (layers F.Cu-L1 F.Paste F.Mask)
      (net 3 Vdd))
    (pad 2 smd rect (at -4.445 5) (size 0.762 1.27) (layers F.Cu-L1 F.Paste F.Mask)
      (net 58 12MHz))
    (pad 3 smd rect (at -3.175 5) (size 0.762 1.27) (layers F.Cu-L1 F.Paste F.Mask))
    (pad 4 smd rect (at -1.905 5) (size 0.762 1.27) (layers F.Cu-L1 F.Paste F.Mask)
      (net 86 "Net-(R52-Pad1)"))
    (pad 5 smd rect (at -0.635 5) (size 0.762 1.27) (layers F.Cu-L1 F.Paste F.Mask))
    (pad 6 smd rect (at 0.635 5) (size 0.762 1.27) (layers F.Cu-L1 F.Paste F.Mask))
    (pad 7 smd rect (at 1.905 5) (size 0.762 1.27) (layers F.Cu-L1 F.Paste F.Mask))
    (pad 8 smd rect (at 3.175 5) (size 0.762 1.27) (layers F.Cu-L1 F.Paste F.Mask))
    (pad 9 smd rect (at 4.445 5) (size 0.762 1.27) (layers F.Cu-L1 F.Paste F.Mask))
    (pad 10 smd rect (at 5.715 5) (size 0.762 1.27) (layers F.Cu-L1 F.Paste F.Mask)
      (net 97 "Net-(R55-Pad1)"))
    (pad 20 smd rect (at -5.715 -5) (size 0.762 1.27) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 19 smd rect (at -4.445 -5) (size 0.762 1.27) (layers F.Cu-L1 F.Paste F.Mask)
      (net 52 /D+))
    (pad 18 smd rect (at -3.175 -5) (size 0.762 1.27) (layers F.Cu-L1 F.Paste F.Mask)
      (net 51 /D-))
    (pad 17 smd rect (at -1.905 -5) (size 0.762 1.27) (layers F.Cu-L1 F.Paste F.Mask)
      (net 3 Vdd))
    (pad 16 smd rect (at -0.635 -5) (size 0.762 1.27) (layers F.Cu-L1 F.Paste F.Mask))
    (pad 15 smd rect (at 0.635 -5) (size 0.762 1.27) (layers F.Cu-L1 F.Paste F.Mask))
    (pad 14 smd rect (at 1.905 -5) (size 0.762 1.27) (layers F.Cu-L1 F.Paste F.Mask))
    (pad 13 smd rect (at 3.175 -5) (size 0.762 1.27) (layers F.Cu-L1 F.Paste F.Mask))
    (pad 12 smd rect (at 4.445 -5) (size 0.762 1.27) (layers F.Cu-L1 F.Paste F.Mask)
      (net 98 RXD))
    (pad 11 smd rect (at 5.715 -5) (size 0.762 1.27) (layers F.Cu-L1 F.Paste F.Mask))
    (model smd/cms_soj24.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.6 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 5843830A)
    (at 137.395 107.85 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 2.5 -0.6 270) (layer F.SilkS))
    (fp_text value 10u (at 2.75 0.55 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 92 SQ4B))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 32 "Net-(C6-Pad2)"))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 58441B1D)
    (at 163.895 88.2 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at -2.525 0.6 270) (layer F.SilkS))
    (fp_text value 10u (at -2.775 -0.6 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 5 AVdd))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 584A3A52)
    (at 130.595 98.55 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C15 (at -0.175 2.4 270) (layer F.SilkS))
    (fp_text value 10u (at -0.1 1.4 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 16 "Net-(C15-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer F.Cu-L1) (tedit 5821A9FA)
    (at 97.095 94)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C21 (at -2.8 0.5) (layer F.SilkS))
    (fp_text value 10u (at -2.8 -0.75) (layer F.SilkS))
    (pad 1 smd rect (at -1 0) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 3 Vdd))
    (pad 2 smd rect (at 1 0) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 5833ADA0)
    (at 89.445 104.9 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 2.4 -0.6 180) (layer F.SilkS))
    (fp_text value 18 (at 2.4 0.5 180) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 180) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 7 V+))
    (pad 2 smd rect (at 1 0 180) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 14 "Net-(C11-Pad1)"))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 5833AD95)
    (at 89.245 112.85 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at 2.85 -0.65 180) (layer F.SilkS))
    (fp_text value 18 (at 2.5 0.4 180) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 180) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 8 V-))
    (pad 2 smd rect (at 1 0 180) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 18 "Net-(C18-Pad2)"))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer B.Cu-L4) (tedit 5843BE15)
    (at 152.145 93.875)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C44 (at 0.2 -2.525) (layer B.SilkS))
    (fp_text value 15p (at 0.05 -1.475) (layer B.SilkS))
    (pad 1 smd rect (at -1 0) (size 1 1.3) (layers B.Cu-L4 B.Paste B.Mask)
      (net 58 12MHz))
    (pad 2 smd rect (at 1 0) (size 1 1.3) (layers B.Cu-L4 B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:C_0805 (layer B.Cu-L4) (tedit 5843BE22)
    (at 152.12 96.45)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf), AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C45 (at -0.125 2.875) (layer B.SilkS))
    (fp_text value 15p (at -0.1 1.575) (layer B.SilkS))
    (pad 1 smd rect (at -1 0) (size 1 1.3) (layers B.Cu-L4 B.Paste B.Mask)
      (net 85 "Net-(C45-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.3) (layers B.Cu-L4 B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 5848DBDA)
    (at 120.895 99.5 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R52 (at 2.78 0.62 90) (layer F.SilkS))
    (fp_text value 10K (at 2.8 -0.48 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 86 "Net-(R52-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 3 Vdd))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:myUSB_MINI_B (layer F.Cu-L1) (tedit 58351E8A)
    (at 79.345 87.8)
    (descr "USB Mini-B 5-pin SMD connector")
    (tags "USB, Mini-B, connector")
    (fp_text reference CON1 (at -2.805 6.625) (layer F.SilkS) hide)
    (fp_text value USB-MINI-B (at -0.275 -6.225) (layer F.SilkS) hide)
    (pad 1 smd rect (at 3.8 -1.6002) (size 3 0.50038) (layers F.Cu-L1 F.Paste F.Mask)
      (net 96 VUSB))
    (pad 2 smd rect (at 3.8 -0.8001) (size 3 0.50038) (layers F.Cu-L1 F.Paste F.Mask)
      (net 51 /D-))
    (pad 3 smd rect (at 3.8 0) (size 3 0.50038) (layers F.Cu-L1 F.Paste F.Mask)
      (net 52 /D+))
    (pad 4 smd rect (at 3.8 0.8001) (size 3 0.50038) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 3.8 1.6002) (size 3 0.50038) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 3.35026 -4.45008) (size 2.49936 1.99898) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -2.14884 -4.45008) (size 2.49936 1.99898) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 3.35026 4.45008) (size 2.49936 1.99898) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -2.14884 4.45008) (size 2.49936 1.99898) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at 0.8509 -2.19964) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0.8509 2.19964) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 5843E4B2)
    (at 134.795 107.89 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R53 (at 2.85 -0.55 270) (layer F.SilkS))
    (fp_text value 5K1 (at 2.75 0.48 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 93 SQ4A))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 92 SQ4B))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 584A3851)
    (at 132.195 107.875 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R54 (at 2.85 -0.55 270) (layer F.SilkS))
    (fp_text value 100K (at 3.175 0.4 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 34 SQ4))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 92 SQ4B))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMDCAP:C_1206 (layer F.Cu-L1) (tedit 5848E9B1)
    (at 88.955 107.5 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C12 (at 3.38 -0.73 180) (layer F.SilkS))
    (fp_text value 22u (at 3.33 0.25 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 7 V+))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD/C_1206N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMDCAP:C_1206 (layer F.Cu-L1) (tedit 5844D49E)
    (at 88.955 110.2 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C19 (at 3.25 -0.77 180) (layer F.SilkS))
    (fp_text value 22u (at 3.18 0.2 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers F.Cu-L1 F.Paste F.Mask)
      (net 8 V-))
    (model Capacitors_SMD/C_1206N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 584A385F)
    (at 126.465 99.52 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R55 (at -2.845 -0.48 270) (layer F.SilkS))
    (fp_text value 1 (at -2.245 0.545 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 97 "Net-(R55-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 99 TXD))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:myTestPoint (layer F.Cu-L1) (tedit 5848E439)
    (at 92.035 108.2)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference TP3 (at 0.65 2.25) (layer F.SilkS) hide)
    (fp_text value V+ (at 2.4 -0.3) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 7 V+))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:myTestPoint (layer F.Cu-L1) (tedit 5848E3F4)
    (at 92.035 112.43)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference TP5 (at 0.65 2.25) (layer F.SilkS) hide)
    (fp_text value V- (at 2.4 -0.3) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 8 V-))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:R_0805 (layer F.Cu-L1) (tedit 585109BA)
    (at 137.72 114.95 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R56 (at 2.75 -0.55 270) (layer F.SilkS))
    (fp_text value 5K1 (at 2.8 0.575 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 32 "Net-(C6-Pad2)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.3) (layers F.Cu-L1 F.Paste F.Mask)
      (net 101 "Net-(C7-Pad1)"))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:fiducial placed (layer F.Cu-L1) (tedit 58521477)
    (at 107.995 117.9)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference FM1 (at 0 -2.286) (layer F.SilkS) hide)
    (fp_text value V- (at 0.35 -1.35) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 2 2) (layers F.Cu-L1 F.Paste F.Mask)
      (clearance 1))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:fiducial placed (layer F.Cu-L1) (tedit 5852148E)
    (at 196.995 89.9)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference FM2 (at 0 -2.286) (layer F.SilkS) hide)
    (fp_text value V- (at 0.35 -1.35) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 2 2) (layers F.Cu-L1 F.Paste F.Mask)
      (clearance 1))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:fiducial placed (layer F.Cu-L1) (tedit 58521506)
    (at 180.995 86.9)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference FM3 (at 0 -2.286) (layer F.SilkS) hide)
    (fp_text value V- (at 0.35 -1.35) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 2 2) (layers F.Cu-L1 F.Paste F.Mask)
      (clearance 1))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text GND (at 84.995 111.875) (layer B.SilkS))
  (gr_text VDD (at 84.82 117.175) (layer B.SilkS))
  (gr_text TX (at 84.62 114.725) (layer B.SilkS))
  (gr_text RX (at 84.695 115.95) (layer B.SilkS))
  (gr_text VDD (at 175.295 92.6) (layer B.SilkS))
  (gr_text GND (at 175.27 91.275) (layer B.SilkS))
  (gr_text CS1 (at 175.275 90.02) (layer B.SilkS))
  (gr_text CS2 (at 175.265 88.8) (layer B.SilkS))
  (gr_text SCK (at 175.295 87.525) (layer B.SilkS))
  (gr_text SDO (at 175.245 86.2) (layer B.SilkS))
  (gr_text SDI (at 175.545 84.975) (layer B.SilkS))
  (gr_text PGD (at 175.345 83.75) (layer B.SilkS))
  (gr_line (start 144.995 119.9) (end 74.995 119.9) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text OD1 (at 120.315 114.8) (layer B.SilkS))
  (gr_text GND (at 198.02 101.625 90) (layer F.SilkS))
  (gr_text GND (at 197.97 109.325 90) (layer F.SilkS))
  (gr_text VR+ (at 198.07 111.825 90) (layer F.SilkS))
  (gr_text VUSB (at 190.645 86.75) (layer F.SilkS))
  (gr_text SDA (at 197.97 106.75 90) (layer F.SilkS))
  (gr_text VR- (at 197.995 116.7 90) (layer F.SilkS))
  (gr_line (start 198.995 119.9) (end 194.995 119.9) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 198.995 81.9) (end 198.995 119.9) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.995 81.9) (end 198.995 81.9) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.995 119.9) (end 74.995 81.9) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 194.995 119.9) (end 144.995 119.9) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text GND (at 116.675 114.89) (layer B.SilkS))
  (gr_text +5V (at 197.995 99.05 90) (layer F.SilkS))
  (gr_text GND (at 198.07 114.4 90) (layer F.SilkS))
  (gr_text SCL (at 198.045 104.1 90) (layer F.SilkS))
  (gr_text GND (at 173.815 115.01) (layer B.SilkS))
  (gr_text MIC (at 191.215 114.82) (layer B.SilkS))
  (gr_text GND (at 180.745 114.8) (layer B.SilkS))
  (gr_text CH3 (at 184.305 114.8) (layer B.SilkS))
  (gr_text Rg (at 187.795 114.5) (layer B.SilkS))
  (gr_text CH2 (at 177.415 114.85) (layer B.SilkS))
  (gr_text GND (at 159.695 114.93) (layer B.SilkS))
  (gr_text CH1 (at 170.245 114.82) (layer B.SilkS))
  (gr_text ID1 (at 163.215 114.82) (layer B.SilkS))
  (gr_text GND (at 166.745 114.86) (layer B.SilkS))
  (gr_text SEN (at 156.235 114.84) (layer B.SilkS))
  (gr_text CAP (at 152.715 114.86) (layer B.SilkS))
  (gr_text GND (at 109.755 114.88) (layer B.SilkS))
  (gr_text PV1 (at 92.165 114.98) (layer B.SilkS))
  (gr_text PV2 (at 99.265 115.01) (layer B.SilkS))
  (gr_text WG (at 127.285 114.86) (layer B.SilkS))
  (gr_text WGB (at 123.855 114.94) (layer B.SilkS))
  (gr_text GND (at 95.795 114.96) (layer B.SilkS))
  (gr_text GND (at 102.745 114.91) (layer B.SilkS))
  (gr_text CLR (at 84.945 113.375) (layer B.SilkS))
  (gr_text SQ2 (at 113.225 114.87) (layer B.SilkS))
  (gr_text SQ1 (at 106.255 114.81) (layer B.SilkS))
  (gr_text 7660 (at 80.995 107.525 270) (layer F.SilkS))
  (gr_text LM324 (at 99.42 109.025 180) (layer F.SilkS))
  (gr_text "ExpEYES-2017\n04JAN2017\n" (at 154.77 89.95) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer L2-GND) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.12)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 198.62 93.725) (xy 188.745 93.725) (xy 188.72 82.325) (xy 104.545 82.65) (xy 104.77 89.75)
        (xy 86.22 89.75) (xy 86.17 82.6) (xy 75.17 82.425) (xy 75.17 119.65) (xy 198.845 119.675)
        (xy 198.62 93.725)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu-L1) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.12)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 198.745 93.75) (xy 188.82 93.675) (xy 188.82 82.4) (xy 104.595 82.5) (xy 104.695 89.7)
        (xy 86.42 89.8) (xy 86.295 82.225) (xy 75.17 82.175) (xy 75.145 119.65) (xy 198.72 119.55)
        (xy 198.745 93.75)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu-L4) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.12)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86.245 82.2) (xy 86.445 89.55) (xy 104.495 89.6) (xy 104.57 82.3) (xy 188.82 82.2)
        (xy 188.87 93.675) (xy 198.82 93.7) (xy 198.645 119.35) (xy 75.545 119.4) (xy 75.32 82.175)
        (xy 86.245 82.2)
      )
    )
  )
)
